

**fcgkj ljdkj**

**fcgkj jkT; 'kS{kf.kd vk/kkjHkwr lajpuk fodkl fuxe fyŒ**

BIHAR STATE EDUCATIONAL INFRASTRUCTURE DEVELOPMENT CORPORATION LTD.

**(A Govt. of Bihar Undertaking)**

ISO 9001; 14001; OHSAS 18001

Shiksha Bhawan, Bihar Rashtrabhasha Parishad Campus, Acharya Shivpujan Sahay Path, Saidpur, Patna-800004

Tel. No.: 0612-2660850 ● Fax No.: 0612-2660256

E-mail: [bseidc@gmail.com](mailto:bseidc@gmail.com) ● website: http://www.bseidc.in ● CIN U80301BR2010SGC015859

**nj vkea=.k gsrq vYidkyhu dksVs’ku vkea=.k lwpuk la[;k&05 o"kZ&2020&21**

fcgkj jkT; 'kS{kf.kd vk/kkjHkwr lajpuk fodkl fuxe fyŒ iVuk ds fucaf/kr laosndksa@[;kfr izkIr QeksZa@daifu;ksa ls fnukad%& **26-06-2020** ds vijkgu 03%00 cts rd jkT; ds fofHkUu ftykUrxZr fofHkUu fuekZ.k dk;ksZ esa iz;ksx gsrq PHE ls lacaf/kr dk;ksZ gsrq xSj vuqlwfpr enksa dh vkiwfrZ ,oa vf/k"Bkiu ds fy, fuEukafdr enksa gsrq eqgjcan dksVs’ku v/kh{k.k vfHk;ark] fcgkj jkT; 'kS{kf.kd vk/kkjHkwr lajpuk fodkl fuxe fyŒ] iVuk ds dk;kZy; esa izkIr fd;k tk,xk ,oa mlh fnu vijkgu 03%30 cts dksVs’kunkrkvksa ;k muds vf/kd`r izfrfuf/k;ksa ds le{k [kksyk tk,xkA

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Sl. No.** | **Description of items** | **Qty** | **Unit** | **Rate  In Digits** | **Rate  In Words** |
| 1 | Supplying , installation, testing & commissionong of suitable capacity of and type of submersible pump set (1HP) cabable of clean filtered water from a deep tubewell at oa total head of 30 meter complete with control panel , gate valve , 60 mtr. of neoprane cable etc.(Crompton/KSB make) all complete job as per direction of E/I. | 1 | Each |  |  |
| 2 | Supplying , installation, testing & commissionong of suitable capacity of and type of submersible pump set (3HP) cabable of clean filtered water from a deep tubewell at oa total head of 30 meter complete with control panel , gate valve , 60 mtr. of neoprane cable etc. (Crompton/KSB make) all complete job as per direction of E/I. | 1 | Each |  |  |
| 3 | Supplying , installation, testing & commissionong of suitable capacity of and type of submersible pump set (5HP) cabable of clean filtered water from a deep tubewell at oa total head of 30 meter complete with control panel , gate valve , 60 mtr. of neoprane cable etc. (Crompton/KSB make) all complete job as per direction of E/I. | 1 | Each |  |  |
| 4 | Providing, fitting & fixing of 25 mm CPVC full Way valve all complete job as per direction of E/I. | 1 | Each |  |  |
| 5 | Providing, fitting & fixing of 32 mm CPVC valve all complete job as per direction of E/I. | 1 | Each |  |  |
| 6 | Providing, fitting & fixing of 40 mm CPVC valve all complete job as per direction of E/I. | 1 | Each |  |  |
| 7 | Providing, fitting & fixing of 50 mm CPVC valve all complete job as per direction of E/I. | 1 | Each |  |  |
| 8 | Providing, fitting & fixing of 65 mm CPVC valve all complete job as per direction of E/I. | 1 | Each |  |  |
| 9 | Providing, fitting & fixing of 80 mm CPVC valve all complete job as per direction of E/I. | 1 | Each |  |  |
| 10 | Providing, fitting & fixing of 100 mm CPVC valve all complete job as per direction of E/I. | 1 | Each |  |  |
| 11 | Providing, fitting & fixing of 25 mm CPVC Union all complete job as per direction of E/I. | 1 | Each |  |  |
| 12 | Providing, fitting & fixing of 32 mm CPVC Union all complete job as per direction of E/I. | 1 | Each |  |  |
| 13 | Providing, fitting & fixing of 40 mm CPVC Union all complete job as per direction of E/I. | 1 | Each |  |  |
| 14 | Providing, fitting & fixing of 50 mm CPVC Union all complete job as per direction of E/I. | 1 | Each |  |  |
| 15 | Providing, fitting & fixing of 65 mm CPVC Union all complete job as per direction of E/I. | 1 | Each |  |  |
| 16 | Providing, fitting & fixing of 80 mm CPVC Union all complete job as per direction of E/I. | 1 | Each |  |  |
| 17 | Providing, fitting & fixing of 100 mm CPVC Union all complete job as per direction of E/I. | 1 | Each |  |  |
| 18 | Providing, fitting & fixing of 50 mm CPVC Non Return Valve all complete job as per direction of E/I. | 1 | Each |  |  |
| 19 | Providing, fitting & fixing of 110 mm UPVC Cowl all complete job as per direction of E/I. | 1 | Each |  |  |
| 20 | Providing, fitting & fixing of PVC 110 mm SWR P- Trap Valve all complete job as per direction of E/I. | 1 | Each |  |  |
| 21 | Providing, fitting & fixing of PVC 75 mm SWR P- Trap Valve all complete job as per direction of E/I. | 1 | Each |  |  |
| 22 | Providing, fitting & fixing of PVC Floor Trap 110X110 mm dia all complete job as per direction of E/I. | 1 | Each |  |  |
| 23 | Providing and fixing white vitreous china pedestal type water closet (European type W.C. pan) of Make- Jaquar/ Cera/ Kohler/Marc with seat and lid, 10 litre low level white P.V.C. flushing cistern, including flush pipe, with manually controlled device (handle lever), conforming to IS : 7231, with all fittings and fixtures all complete job as per direction of E/I. | 1 | Each |  |  |
| 24 | Providing and fixing water closet squatting pan (Indian type W.C.pan ) of Make- Make- Jaquar/ Cera/ Kohler/Marc with 100 mm sand cast Iron P or S trap, 10 litre low fixtures complete, including cutting and making good the walls andlevel white P.V.C. flushing cistern, including flush pipe, with manually controlled device (handle lever) conforming to IS : 7231, with all fittings and floors wherever required : White Vitreous china Orissa pattern W.C. pan of size 580x440 mm with integral type foot rests | 1 | Each |  |  |
| 25 | Supplying, storing, handling, shifting, installation, testing and commissioning of CP flxible hose, spray, wall flange of Make- Jaquar/ Cera/ Kohler/Marc with all fittings and fixtures all complete job as per direction of E/I. | 1 | Each |  |  |
| 26 | Providing, fitting & fixing of CP Bib Cock two in one Make- Jaquar/ Cera/ Kohler/Marc all complete job as per direction of E/I. | 1 | Each |  |  |
| 27 | Providing and fixing white vitreous china battery based infrared sensor operated urinal of Make Make- Jaquar/ Cera/ Kohler/Marc of size 610 x 390 x 370 mm having pre & post flushing with water ( 250 ml & 500 ml consumption), having water inlet from back side, including fixing to wall with suitable brackets all complete job as per direction of E/I. | 1 | Each |  |  |
| 28 | Providing and fixing Hand dryer of Make Dolphy/Alpine all complete job as per direction of E/I. | 1 | Each |  |  |
| 29 | Providing and fixing CP Bottle Trap for Wash basin and sink.  Bottle trap 31 mm single piece moulded with height of 270 mm, effective length of tail pipe 260 mm from the centre of the waste coupling 77 mm breadth with 25 mm minimum water seal, weighing not less than 260 gms all complete job as per direction of E/I. | 1 | Each |  |  |
| 30 | Providing and fixing CP liquid soap container 109 mm wide, 125 mm high and 112 mm distance from wall of standard shape with bracket of the same materials with snap fittings of approved quality and colour weighing not less than 105 gms all complete job as per direction of E/I. | 1 | Each |  |  |
| 31 | Providing & fixing CP towel ring trapezoidal shape/ rod of 215 mm long 200 mm wide with minimum distance of 37 mm from wall face with concealed fittings arrangement of approved quality and colour weighing not less than 88 gms all complete job as per direction of E/I. | 1 | Each |  |  |

**fo'ks"k 'krsZ&**

* ;g dksVs’ku flQZ nj fu/kkZj.k gsrq vkeaf=r fd;k x;k gSA
* dksVs’kunkrkvksa dks viuk nj ¼lHkh djksa] GST ,oa <qykbZ O;; ds lkFk½ vad ,oa v{kjksa esa m)`r djuk gksxkA
* fo’ks"k lwpuk ds fy, lwpukiV~V ;k osclkbV [www.prdbihar.gov.in](http://www.prdbihar.gov.in) ,oa [www.bseidc.in](http://www.bseidc.in) ns[ksa vFkok v/kksgLrk{kjh ds dk;kZy; esa dk;kZof/k esa laidZ fd;k tk ldrk gSA

**v/kh{k.k vfHk;ark**

**BSEIDC, iVukA**